"SimpleMouse" Smartcardprogrammer

| Home Projects Mcu (Microcontrollers) "SimpleMouse" Smartcardprogrammer |

"SimpleMouse" Smartcardprogrammer

source: Keule

> > This "SimpleMouse" Smartcardprogrammer can be used to read and write most of all async - Smartcards (Processorcards), including the new "Hornet and +1" DPSC´s in update and reprogramming mode.
> > It is jumper-selectable in either Smartmouse or Phoenix Mode (Reset active hi or low) and Jumper selectable for 3.57 and 6 MHz
> > The "original" Smartmouse gets its power out of the serial port of the Hostcomputer - in this design this "feature" is not implemented because the Hostcomputer can only deliver about 15 mA to the Programmer. This is not enough for older Smartcards. So this design uses an 9V Alkaline Battery 6LR61.
> > To make this design cheap there are no gimmicks like flashing diodes or expensive connectors and switches. You have to solder the 9 or 25 pin serial cable directly the corresponding pads of the PCB.

> > ++++++++++++
> > There is an new/other Layout included. It has some 100R Resistors in
> > the connections to the smartcard, to limit the current in the case
> > of malfunction of the software. Furthermore the Layout is a litte more
> > easier to build at home because the distance between the tracks is
> > bigger....
> > All the following description is also usable for the new layout. Some
> > changes in the partvalues have to be taken directly out of the Top1.gif.
> > The LEDs schould be LowPower....

> > Download the files in zip

> > ++++++++++++
> > JUMPERS
> > SIP1 is for selecting the Clockrate 3.57 or 6MHz
> > SIP 1
> > Shorting pin 1 + 2 -> 3.57 MHz
> > Shorting pin 2 + 3 -> 6 MHz
> > SIP2 is for selecting the type of mode (Smartmouse or Phoenix)
> > SIP 2
> > Shorting pin 1 + 2 -> Smartmouse
> > Shorting pin 2 + 3 -> Phoenix
> > SIP3
> > SIP3 is a Jumperblock which is used as a "Switch" to turn the Battery
> > on an off - or as the connector for an external DC-powersupply.
> > Shorting pin 1+2 -> Power off
> > Shorting pin 2+3 -> Power on
> > Without Jumper you can connect an external DC-Powersupply to this Header:
> > Pin1 -> GND
> > Pin2 -> 9 to 15 Vdc
> > Pin3 -> left open
> > SIP4
> > SIP3 is´nt really a Jumperblock it is the connection to the serial
> > Port of the Hostcomputer.
> > SIP4 9Pin SubD Serial port cable
> > Pin1 -> Pin 5
> > Pin2 -> Pin 2
> > Pin3 -> Pin 3
> > Pin4 -> Pin 1
> > Pin5 -> Pin 7
> > PART LIST
> > ID Comment
> > BT1 9V Block Alkaline
> > C1 22pF RM 5 Keramik
> > C2 22pF RM 5 Keramik
> > C3 22pF RM 5 Keramik
> > C4 22pF RM 5 Keramik
> > C5 100nF RM 5 KDPU
> > C6 100nF RM 5 KDPU
> > C7 1uF RM 2.5 Tantal
> > C8 1uF RM 2.5 Tantal
> > C9 1uF RM 2.5 Tantal
> > C10 1uF RM 2.5 Tantal
> > C11 1u RM 2.5 Tantal
> > C12 100nF RM 5 KDPU
> > C13 100nF RM 5 KDPU
> > C14 47pF RM 5 Keramik
> > C15 1uF RM 2.5 Tantal
> > D1 BAT41 or BAT48 Shottky!!
> > D2 1N4148
> > LD1 LED 3mm red Low Power
> > R1 1M RM 5 Bauform 02/04 1/10W
> > R2 2K2 RM 5 Bauform 02/04 1/10W
> > R3 1M RM 5 Bauform 02/04 1/10W
> > R4 2K2 RM 5 Bauform 02/04 1/10W
> > R5 2K2 RM 5 Bauform 02/04 1/10W
> > R6 2K2 RM 5 Bauform 02/04 1/10W
> > R7 10K RM 5 Bauform 02/04 1/10W
> > SC1 Smartcard Adapter Amphenol Switch opens when Card is inserted!
> > SIP1 Jumperblock 3Pin
> > SIP2 Jumperblock 3Pin
> > SIP3 Jumperblock 3Pin
> > SIP4 Jumperblock 5Pin
> > U1 74HC00
> > U2 MAX 232
> > U3 78L05
> > X1 3.57MHz HC18/U
> > X2 6MHz HC18/U
> > All Rs are 1/10W 4mm for laying mount or 1/4 W for standing mount.
> > REMARKS
> > It is very important for this design to use a Shottky diode for D1.
> > Any other type will definitely NOT work!
> > Look for the right polarity of the tantalum condensators! The
> > MAX232 includes a so called chargepump and generates positive an
> > negative Voltages respect to ground. So it is possible that the
> > positive pole of an condensator is connected to ground - this is
> > NOT wrong!
> > For Mounting the Battery and fasten the serial cabel drill bigger
> > holes at the corresponding points and use cablestrips.
> > The enclosed Tiff´s have a resolution of 400 dpi.
> > ++++++++++++++++++
> > Das Layout5 ist um folgende Bauteile erweitert
> > IC NE555
> > R 10K
> > R 120K
> > C 1uF Elko
> > Taster 1 x UM
> > Der Taster muss in Ruhestellung Masse Stromversorgung mit Masse Board verbinden, gedrückter Position PIN3 NE555 MIT Masse Board.
> > Durch diese einfache Erweiterung können Karten genullt bzw. reanimiert werden ohne das raus-rein Spiel, welches die Karte unnütz strapaziert.
> > Greetz Keule-

| Search Site | WWW Search | Upload Center | Support us | Advertising | FAQ | Profile | Books | Gadgets | Add your link here
| Free Schematics Search Engine | Electronic Kits | Best Buy Mobile Phones | Pricemate
| Electronics-lab.com © 2002-2004 Any logo, trademark and project represented here are property of their respective owner